mSupply Desktop Integration

Prerequisites

Minimum (BlueMaestro syncing with mSupply Desktop):

mSupply cold chain app version: 0.4.2 recommended

mSupply Desktop version: V5-04-00 or higher recommended

Laird Sensor Support

mSupply cold chain app version: 0.5.0-rc0

Minimum mSupply Desktop version: V5-07-00-RC41

mSupply Desktop Setup Steps

Instructions on the server side setup are located on the mSupply Desktop documentation site.

mSupply Cold Chain Setup Steps

Navigate to SETTINGS

Navigate to SYNC SETTINGS

Put in your store credentials under USERNAME and PASSWORD

Add Urls

Authentication - example: http://192.168.4.3:8080/coldchain/v1/login

Temperature-log - example: http://192.168.4.3:8080/coldchain/v1/temperature-log

Temperature-breach - example: http://192.168.4.3:8080/coldchain/v1/temperature-breach

Sensor - example: http://192.168.4.3:8080/coldchain/v1/sensor

The tablet will push data into the server every 1-2 minutes