mSupply Integration

Prerequisites

Minimum (BlueMaestro syncing with mSupply Desktop):

mSupply cold chain app version: 0.4.2 recommended

mSupply Desktop version: V5-04-00 or higher recommended

Laird Sensor Support

mSupply cold chain app version: 0.5.0-rc0

Minimum mSupply Desktop version: V5-07-00-RC41